|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SL.NO** | **EQUIPMENT** | **TON** | **SCHEDULE** | **DURATION** | **MANPOWER** | **TOTAL Nos** |
| **1** | **Hyster Forklift** | **13** | **2 WEEKS CHECK UP**  **6 WEEKS NORMAL MAINTENANCE**  **48 WEEKS FULL MAINTENANCE** | **40 min**  **1 hr**  **3hr** | **1rig/ 1mec / 1op**  **1rig /2mec / 1op**  **1 rig/ 2mec / 1op** | **2** |
| **2** | **Hyster Forklift (OLD)** | **25** | **1 WEEKS CHECK UP**  **6 WEEKS NORMAL MAINTENANCE**  **48 WEEKS FULL MAINTENANCE** | **40 min**  **1 hr**  **3hr** | **1rig/ 1mec / 1op**  **1rig /2mec / 1op**  **1 rig/ 2mec / 1op** | **2** |
| **3** | **Hyster Forklift (NEW)** | **25** | **1 WEEKS CHECK UP**  **3 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **40 min**  **1 hr**  **3hr** | **1rig/ 1mec / 1op**  **1rig /2mec / 1op**  **1 rig/ 2mec / 1op** | **4** |
| **4** | **Hyster Forklift** | **50** | **1 WEEKS CHECK UP**  **6 WEEKS NORMAL MAINTENANCE**  **48 WEEKS FULL MAINTENANCE** | **40 min**  **1 hr**  **3hr** | **1rig/ 1mec / 1op**  **1rig /2mec / 1op**  **1 rig/ 3mec / 1op** | **2** |
| **5** | **KONECRANE Forklift** | **25** | **1 WEEKS CHECK UP**  **6 WEEKS NORMAL MAINTENANCE**  **48 WEEKS FULL MAINTENANCE** | **40 min**  **1 hr**  **3hr** | **1rig/ 1mec / 1op**  **1rig /2mec / 1op**  **1 rig/ 3mec / 1op** | **4** |
| **6** | **TEREX RT CRANE** | **63** | **1 WEEK CHECK UP**  **8 WEEKS NORMAL MAINTENANCE**  **64 WEEKS FULL MAINTENANCE** | **30 min**  **2 hr**  **3.5 hr** | **1mec / 1op**  **1rig / 2mec / 1 op**  **1 rig/ 3mec / 1op** | **3** |
| **7** | **GROVE RT CRANE** | **63** | **1 WEEK CHECK UP**  **8 WEEKS NORMAL MAINTENANCE**  **64 WEEKS FULL MAINTENANCE** | **30 min**  **2 hr**  **3.5 hr** | **1mec / 1op**  **1rig / 2mec / 1 op**  **1 rig/ 3mec / 1op** | **5** |
| **8** | **TEREX RT CRANE** | **45** | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **2 hr**  **3.5 hr** | **1mec / 1op**  **1rig / 2mec / 1 op**  **1 rig/ 3mec / 1op** | **2** |
| **9** | **GROVE RT CRANE** | **45** | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **2 hr**  **3.5 hr** | **1mec / 1op**  **1rig / 2mec / 1 op**  **1 rig/ 3mec / 1op** | **12** |
| **10** | **GROVE RT CRANE** | **35** | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **2 hr**  **3.5 hr** | **1mec / 1op**  **1rig / 2mec / 1 op**  **1 rig/ 3mec / 1op** | **2** |
| **11** | **GROVE RT CRANE** | **30** | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **2 hr**  **3.5 hr** | **1mec / 1op**  **1rig / 2mec / 1 op**  **1 rig/ 3mec / 1op** | **5** |
| **12** | **TIPPER - SCANIA** |  | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **1 hr**  **2.5 hr** | **1mec / 1 op**  **1mec / 1 op**  **2mec / 1 op** | **2** |
| **13** | **TIPPER - HINO** |  | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **1 hr**  **2.5 hr** | **1mec / 1 op**  **1mec / 1 op**  **2mec / 1 op** | **3** |
| **14** | **CARGO TRUCK WITH HYDRAULIC 5 TON CRANE WITH OUTRIGGERS - MAN** |  | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **1 hr**  **2.5 hr** | **1mec / 1 op**  **1mec / 1 op**  **2mec / 1 op** | **8** |
| **15** | **CARGO TRUCK WITH HYDRAULIC 3 TON CRANE WITH OUTRIGGERS - HINO** |  | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **1 hr**  **2.5 hr** | **1mec / 1 op**  **1mec / 1 op**  **2mec / 1 op** | **2** |
| **16** | **DIESEL TANKER - MAN** |  | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **1 hr**  **2.5 hr** | **1mec / 1 op**  **1mec / 1 op**  **2mec / 1 op** | **2** |
| **17** | **TRUCK WITH CARGO BODY – LUBE TRUCK – MAN/BENZ** |  | **1 WEEK CHECK UP**  **4 WEEKS NORMAL MAINTENANCE**  **24 WEEKS FULL MAINTENANCE** | **30 min**  **1 hr**  **2.5 hr** | **1mec / 1 op**  **1mec / 1 op**  **2mec / 1 op** | **2** |